(footprint "CONN-TH_KH-A01M-A-M2-6P"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 0 0)
		(layer "F.SilkS")
		(uuid "c1338bd9-5a35-44af-b07c-4fe1f4cde0e3")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" ""
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "a4ef7206-c676-4708-a54e-70d0bef2060f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "33fc9706-337c-4212-aa0e-162ce89e261b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "b3fd02d1-c7bc-42d3-aa97-5979bfadebf6")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_line
		(start -8.827 -2.159)
		(end -8.827 -1.8525)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "f14da8d3-39f8-419a-a6c0-35c18670763b")
	)
	(fp_line
		(start -8.827 1.8525)
		(end -8.827 8.382)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "9ee50bf6-b105-4487-a690-9a8f64876027")
	)
	(fp_line
		(start -8.827 2.54)
		(end -8.827 3.175)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "e3e2e73f-2d7f-4f1c-b5b9-43d5cdde2b1a")
	)
	(fp_line
		(start -8.827 8.382)
		(end 8.827 8.382)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "0161b809-1ddd-49e6-8203-bb6fd599e6a7")
	)
	(fp_line
		(start 8.827 -2.159)
		(end -8.827 -2.159)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "b957aabd-2df7-45fd-a449-65e9797e37eb")
	)
	(fp_line
		(start 8.827 -1.8525)
		(end 8.827 -2.159)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "20f117c7-faf8-47ee-b16f-b238e06ed2b9")
	)
	(fp_line
		(start 8.827 2.54)
		(end 8.827 1.8525)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "f3769f82-9ad7-4c51-bc1c-57095904954a")
	)
	(fp_line
		(start 8.827 2.54)
		(end 8.827 8.382)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "9d8cf333-092b-409f-86ab-7bef5cb020b8")
	)
	(fp_line
		(start -8.825 2.54)
		(end 8.827 2.54)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "4f1438ef-e05e-42f6-9351-962df4aec191")
	)
	(fp_line
		(start -8.825 4.191)
		(end -8.825 2.54)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "945f6d0c-daa2-4642-9d74-631e75b278f8")
	)
	(fp_line
		(start 8.827 2.54)
		(end 8.827 4.318)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "f0b75bfb-7c94-43dd-b0e4-76ba92335520")
	)
	(pad "1" thru_hole rect
		(at -5 0)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "fbdf7b2c-492c-4fbc-aa19-826a3f3f7c72")
	)
	(pad "2" thru_hole circle
		(at -3 0)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "00981cbd-43ce-42fe-afa2-df8d4131d264")
	)
	(pad "3" thru_hole circle
		(at -1 0)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "10d4ce25-448f-4433-8758-3f0301281734")
	)
	(pad "4" thru_hole circle
		(at 1 0)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "1ddec1b2-0a8a-4584-abd9-a0f0607686ef")
	)
	(pad "5" thru_hole circle
		(at 3 0)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "8c4bca8a-9649-4f9b-ad0d-26b23ddcc6ad")
	)
	(pad "6" thru_hole circle
		(at 5 0)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "1d6aa054-2e71-4da1-a749-e0adc0b0081d")
	)
	(pad "7" thru_hole circle
		(at 8.125 0)
		(size 3.5 3.5)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "1f238ddb-5a9a-4af2-adc8-bfef4dc5d059")
	)
	(pad "8" thru_hole circle
		(at -8.125 0)
		(size 3.5 3.5)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "26cfc32f-b744-45a8-92d3-4a00c5322ee5")
	)
	(embedded_fonts no)
)
