(footprint "CONN-TH_SMTSOM2.550BTR_C5301778"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 0 0)
		(layer "F.SilkS")
		(uuid "74e38aca-ae8e-4a94-9b45-9d8352e2d3cd")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" ""
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "6a10ac9e-27bd-4d9f-8ee2-1563f1930c7c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "ccc8a9db-768d-48c6-9435-5b2da3486ec6")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "7aa849c7-8016-4df4-89f7-7ca1ce31b2af")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "JLC_3DModel_Q" "d083a49ffadd43d38c30589efc30b4de"
		(at 0 0 0)
		(layer "Cmts.User")
		(hide yes)
		(uuid "495c34cf-89ac-4c18-ba92-3b9a24d7390c")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "JLC_3D_Size" "5.56 5.561"
		(at 0 0 0)
		(layer "Cmts.User")
		(hide yes)
		(uuid "1a411818-6931-4cda-8c64-b9f77b38c0e0")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 6.5 6.5)
		(drill 4.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "83e40d56-f903-4a97-a040-6948c61588c8")
	)
	(embedded_fonts no)
	(model "${KIPRJMOD}/EASYEDA_MODELS/CONN-TH_SMTSOM2.550BTR_C5301778.step"
		(offset
			(xyz 0 0 -1.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -0 -0 -0)
		)
	)
)
