(footprint "CONN-TH_SMTSOM2.550BTR_C5301778"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 0 0)
		(layer "F.SilkS")
		(uuid "b99ff091-777e-4f2c-998a-318d001faee0")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" ""
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "6ceeb040-c57c-4238-8da8-4d555aa063f2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "64026a4a-f5e1-44d2-ad85-fb26ce932116")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "42858213-6210-43e6-bc9e-dda5d9732c43")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "JLC_3DModel_Q" "d083a49ffadd43d38c30589efc30b4de"
		(at 0 0 0)
		(layer "Cmts.User")
		(hide yes)
		(uuid "f97e147c-7527-4c37-b445-34b65d3d21b9")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "JLC_3D_Size" "5.56 5.561"
		(at 0 0 0)
		(layer "Cmts.User")
		(hide yes)
		(uuid "b6a59eda-0c28-4037-a0ce-7a5e7e5ffa6e")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 6.5 6.5)
		(drill 4.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "6cddbb30-cb8e-4132-bb2f-f0f4fef20b48")
	)
	(embedded_fonts no)
	(model "${KIPRJMOD}/EASYEDA_MODELS/CONN-TH_SMTSOM2.550BTR_C5301778.step"
		(offset
			(xyz 0 0 -1.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -0 -0 -0)
		)
	)
)
