(footprint "batt_con_nec"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 0 0)
		(layer "F.SilkS")
		(uuid "aba9a47c-c9a1-4d14-b4c8-6fe011207b0b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" ""
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "66ab3a5c-4852-4fa9-8bae-c518b6653b3a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "5cba0737-e5d8-4b10-bc53-6813dc77217a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "2b901cd2-0363-41bf-9376-21d102d31ea7")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_line
		(start -8.5 -2.25)
		(end -8.5 1.25)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "dc47aab3-cf8c-4fd1-9638-9d1adb9b23b9")
	)
	(fp_line
		(start -8.5 1.25)
		(end 8.5 1.25)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "4c5464b7-5c84-4124-b468-bdb084f3f7cf")
	)
	(fp_line
		(start 8.5 -2.25)
		(end -8.5 -2.25)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "62ff6dc7-bd08-4862-a1d2-ac622d6eb75b")
	)
	(fp_line
		(start 8.5 1.25)
		(end 8.5 -2.25)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "4c7b34e9-cba6-42d1-a0ed-f4d651ccc2ff")
	)
	(fp_line
		(start -6.5 -6.5)
		(end -6.5 -2.25)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "ea8a73a2-f9e4-4a8b-9142-aa1041c58418")
	)
	(fp_line
		(start -6.25 -6.75)
		(end -6.5 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "0b17a581-7ab3-4f08-bc7b-c784bf8b6578")
	)
	(fp_line
		(start -6 -6.5)
		(end -6.25 -6.75)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "f481c68c-5736-46b4-8854-127fc305d87e")
	)
	(fp_line
		(start -5.988 -6.5)
		(end -6 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "ade09567-d355-43ec-a4c5-7e52b0dbd5d8")
	)
	(fp_line
		(start -5.988 -2.25)
		(end -5.988 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "4ebac33d-f2f1-41dd-b852-e0cf648345b1")
	)
	(fp_line
		(start -4 -6.5)
		(end -4 -2.25)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "f45afed0-c09b-4272-8a6c-73161dd53cca")
	)
	(fp_line
		(start -3.75 -6.75)
		(end -4 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "96bbcdcd-c7ab-4eb0-af84-77270f8bc11b")
	)
	(fp_line
		(start -3.5 -6.5)
		(end -3.75 -6.75)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "5d8b34aa-510f-46de-9242-66c9c850152a")
	)
	(fp_line
		(start -3.488 -6.5)
		(end -3.5 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "a7da196d-28b8-456d-ba62-617755167183")
	)
	(fp_line
		(start -3.488 -2.25)
		(end -3.488 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "29db5a90-1bc8-4454-97dd-eef7fa5ba9e6")
	)
	(fp_line
		(start -1.5 -6.5)
		(end -1.5 -2.25)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "19974770-36ea-40a8-996e-533cf9c292d4")
	)
	(fp_line
		(start -1.25 -6.75)
		(end -1.5 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "98472b39-4dfd-4ffe-90f6-39e2151c40a3")
	)
	(fp_line
		(start -1 -6.5)
		(end -1.25 -6.75)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "93fdb5b8-b727-4cc1-bc8f-15d05b0844d4")
	)
	(fp_line
		(start -0.988 -6.5)
		(end -1 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "52fbb2b9-49a0-4f3d-b037-21a9bc3477ff")
	)
	(fp_line
		(start -0.988 -2.25)
		(end -0.988 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "5dc54913-168e-46e3-baa4-5c477a833b6a")
	)
	(fp_line
		(start 1 -6.5)
		(end 1 -2.25)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "6d913e88-335a-4c96-ad6e-4f7a0f14c837")
	)
	(fp_line
		(start 1.25 -6.75)
		(end 1 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "208694c0-f0e7-42b2-b50f-d3acddf43a46")
	)
	(fp_line
		(start 1.5 -6.5)
		(end 1.25 -6.75)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "5faa053f-d1ae-4f71-9cdc-01da6543e46e")
	)
	(fp_line
		(start 1.512 -6.5)
		(end 1.5 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "8dac9d38-b721-4631-aa8e-d4b792e9d8ea")
	)
	(fp_line
		(start 1.512 -2.25)
		(end 1.512 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "bdda105b-f963-4b4e-aa1a-d57ec4e213f4")
	)
	(fp_line
		(start 3.5 -6.5)
		(end 3.5 -2.25)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "34b56452-bc90-483a-bd3c-9a991ca8cd22")
	)
	(fp_line
		(start 3.75 -6.75)
		(end 3.5 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "4e252b09-62ef-4637-b4cf-20c30c3921ad")
	)
	(fp_line
		(start 4 -6.5)
		(end 3.75 -6.75)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "e65d99b7-39d3-4fd3-877d-ab4326294493")
	)
	(fp_line
		(start 4.012 -6.5)
		(end 4 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "aa73573a-0102-4876-af81-fd31e9512835")
	)
	(fp_line
		(start 4.012 -2.25)
		(end 4.012 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "105386fc-2cc6-4ab5-bc6b-9cb7c1830ef1")
	)
	(fp_line
		(start 6 -6.5)
		(end 6 -2.25)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "fdd24394-c96e-46e4-9557-a5f30aec712c")
	)
	(fp_line
		(start 6.25 -6.75)
		(end 6 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "9b582363-95a7-47f4-8ea1-ccbb7e024fab")
	)
	(fp_line
		(start 6.5 -6.5)
		(end 6.25 -6.75)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "ed2c3cb5-16ca-4893-8232-4add5594ef0f")
	)
	(fp_line
		(start 6.512 -6.5)
		(end 6.5 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "6e0cc552-d2ff-4dea-bdf9-116112976085")
	)
	(fp_line
		(start 6.512 -2.25)
		(end 6.512 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "096978ca-d844-4a21-9489-14e6505bfbc5")
	)
	(pad "1" thru_hole circle
		(at 6.25 0)
		(size 1.65 1.65)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "dfa075c1-3280-446e-bebd-a69e3199bfd6")
	)
	(pad "2" thru_hole circle
		(at 3.75 0)
		(size 1.65 1.65)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "e3b2a588-c954-4cd8-894b-a7ad1655717b")
	)
	(pad "3" thru_hole circle
		(at 1.25 0)
		(size 1.65 1.65)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "c001a116-1315-4acb-a621-86f28de736c7")
	)
	(pad "4" thru_hole circle
		(at -1.25 0)
		(size 1.65 1.65)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "b876e7e6-41ad-418e-b93b-3f6b2f0a5995")
	)
	(pad "5" thru_hole circle
		(at -3.75 0)
		(size 1.65 1.65)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "2099468e-bf42-4c29-bf44-6168ac0888ae")
	)
	(pad "6" thru_hole circle
		(at -6.25 0)
		(size 1.65 1.65)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "91d681e0-f9a2-4e84-b61f-8ef115622191")
	)
	(embedded_fonts no)
)
