(footprint "batt_con_nec"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 0 0)
		(layer "F.SilkS")
		(uuid "8165df0f-8dc3-455e-958c-71b0976a9db0")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" ""
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "c68d7bf5-8c38-4634-8a11-285848b94a3e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "7b1e9ee6-7dc6-466b-b394-925191077c96")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "31362161-e87f-4846-a6eb-53f1d767ba90")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_line
		(start -8.5 -2.25)
		(end -8.5 1.25)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "3213cd1e-95d9-478f-a934-c351cc3389e8")
	)
	(fp_line
		(start -8.5 1.25)
		(end 8.5 1.25)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "6409f12f-810a-4a4c-90c3-dff0800c2853")
	)
	(fp_line
		(start 8.5 -2.25)
		(end -8.5 -2.25)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "ebccb9b4-f190-4a43-a642-92174e89d053")
	)
	(fp_line
		(start 8.5 1.25)
		(end 8.5 -2.25)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "89b331ba-44a4-43de-9b1b-640e240c266f")
	)
	(fp_line
		(start -6.5 -6.5)
		(end -6.5 -2.25)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "df784281-9ae3-4abd-bc17-aa8b5b2f37c8")
	)
	(fp_line
		(start -6.25 -6.75)
		(end -6.5 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "821faab4-9ff0-45f0-9d88-a155fba5ca2c")
	)
	(fp_line
		(start -6 -6.5)
		(end -6.25 -6.75)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "a3ed76e2-3bf9-49df-ae92-d71e7a6951f7")
	)
	(fp_line
		(start -5.988 -6.5)
		(end -6 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "96088be4-181d-4411-99f6-9d9f334c9adf")
	)
	(fp_line
		(start -5.988 -2.25)
		(end -5.988 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "081843e5-30c8-4246-8b32-0882560f32f0")
	)
	(fp_line
		(start -4 -6.5)
		(end -4 -2.25)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "87dc90e4-32b6-4776-be62-8841419d3220")
	)
	(fp_line
		(start -3.75 -6.75)
		(end -4 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "11d873d1-153f-4cda-94d2-832b4adc32f0")
	)
	(fp_line
		(start -3.5 -6.5)
		(end -3.75 -6.75)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "a7a40a44-3c7b-4873-bfde-8bae789bce2e")
	)
	(fp_line
		(start -3.488 -6.5)
		(end -3.5 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "4364b45b-db46-41f2-a96e-6344116022c0")
	)
	(fp_line
		(start -3.488 -2.25)
		(end -3.488 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "cf293620-0944-479f-9785-a7dc57ae4b40")
	)
	(fp_line
		(start -1.5 -6.5)
		(end -1.5 -2.25)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "8fbd4b12-c032-4e2f-b7f4-4bcb586ee358")
	)
	(fp_line
		(start -1.25 -6.75)
		(end -1.5 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "b3d1ca21-ca96-4e4f-8dcb-0e6b52bf4e8b")
	)
	(fp_line
		(start -1 -6.5)
		(end -1.25 -6.75)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "e2f254ae-3c22-4670-8183-9fc5643ee046")
	)
	(fp_line
		(start -0.988 -6.5)
		(end -1 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "7dba8213-0e15-4fd0-917c-8624c0a99332")
	)
	(fp_line
		(start -0.988 -2.25)
		(end -0.988 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "1b3e1131-dc5f-4ff8-ac01-73710f07ce7e")
	)
	(fp_line
		(start 1 -6.5)
		(end 1 -2.25)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "a43427d1-c81d-42e8-a076-b849ddd0c17e")
	)
	(fp_line
		(start 1.25 -6.75)
		(end 1 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "3e79b51e-990f-4f3e-bb8e-90ec4ad4e09f")
	)
	(fp_line
		(start 1.5 -6.5)
		(end 1.25 -6.75)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "9bb5de4b-7c67-4b32-bfd4-840df965c81d")
	)
	(fp_line
		(start 1.512 -6.5)
		(end 1.5 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "3d818c30-8b66-4a9b-a8be-d4481951659f")
	)
	(fp_line
		(start 1.512 -2.25)
		(end 1.512 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "167000ef-d7e9-4426-b43b-0f63b1413f9c")
	)
	(fp_line
		(start 3.5 -6.5)
		(end 3.5 -2.25)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "42182c37-8ed4-4f3f-987a-e5bf7a0da535")
	)
	(fp_line
		(start 3.75 -6.75)
		(end 3.5 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "f7b2e6f3-04d8-4651-948a-a38f2c442752")
	)
	(fp_line
		(start 4 -6.5)
		(end 3.75 -6.75)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "1e9675b1-29c8-4b72-8aad-0bae625fbb04")
	)
	(fp_line
		(start 4.012 -6.5)
		(end 4 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "74691b3d-fc41-4fe7-bfcf-3f39338835dc")
	)
	(fp_line
		(start 4.012 -2.25)
		(end 4.012 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "8c75e4c3-258f-452f-b82d-91d29e63d40f")
	)
	(fp_line
		(start 6 -6.5)
		(end 6 -2.25)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "93695308-913e-408b-b0cf-a27d9c6a3c34")
	)
	(fp_line
		(start 6.25 -6.75)
		(end 6 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "01373958-3136-4a88-9740-43e15a75134d")
	)
	(fp_line
		(start 6.5 -6.5)
		(end 6.25 -6.75)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "9cc9a813-105e-4863-b31a-37fc4ef86284")
	)
	(fp_line
		(start 6.512 -6.5)
		(end 6.5 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "59bd948f-87bd-41f7-8057-c5482f3e295d")
	)
	(fp_line
		(start 6.512 -2.25)
		(end 6.512 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "ecb62b77-7584-4880-9185-ae7c0c067cd0")
	)
	(pad "1" thru_hole circle
		(at 6.25 0)
		(size 1.65 1.65)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "9a083e6a-5010-4ae2-bbc0-d595e212d5b2")
	)
	(pad "2" thru_hole circle
		(at 3.75 0)
		(size 1.65 1.65)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "285c2828-6d75-48b4-bba8-56b5857c5923")
	)
	(pad "3" thru_hole circle
		(at 1.25 0)
		(size 1.65 1.65)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "7da5bfa7-26f8-48d5-a936-4167f6fe70d0")
	)
	(pad "4" thru_hole circle
		(at -1.25 0)
		(size 1.65 1.65)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "cf81a34c-3783-48cf-82a5-66b768cdfe49")
	)
	(pad "5" thru_hole circle
		(at -3.75 0)
		(size 1.65 1.65)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "babd8f7f-7578-49c6-a600-862e4380d3f9")
	)
	(pad "6" thru_hole circle
		(at -6.25 0)
		(size 1.65 1.65)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "7d60fa2b-c043-41c0-91c3-91ffcbf65a66")
	)
	(embedded_fonts no)
)
