(footprint "CONN-TH_KH-A01M-A-M2-6P"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 0 0)
		(layer "F.SilkS")
		(uuid "ffd13fb5-aa9d-4236-8e8f-773084a05382")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" ""
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "c634abf5-147f-41a7-bb9a-95958aa47c6b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "cc19c2a9-fcff-43f5-ab09-da48fd27a8f9")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "dbf4bd5a-c0f8-4230-8a3a-0dd738039474")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_line
		(start -8.827 -2.159)
		(end -8.827 -1.8525)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "20995694-1dcc-40f7-bb5c-9ec2d9cc0083")
	)
	(fp_line
		(start -8.827 1.8525)
		(end -8.827 8.382)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "af6e1185-4c53-486a-96e6-3cc9a0468bb4")
	)
	(fp_line
		(start -8.827 2.54)
		(end -8.827 3.175)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "595395bb-e271-4baa-9e51-cd6d9ae86040")
	)
	(fp_line
		(start -8.827 8.382)
		(end 8.827 8.382)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "a08d53aa-027c-46a2-b055-cce6a856c5c6")
	)
	(fp_line
		(start 8.827 -2.159)
		(end -8.827 -2.159)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "ae9d7a95-5d8e-4c7a-860e-7c1514cd80fc")
	)
	(fp_line
		(start 8.827 -1.8525)
		(end 8.827 -2.159)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "5c1e772b-aa43-498b-b792-1d2138ca1d83")
	)
	(fp_line
		(start 8.827 2.54)
		(end 8.827 1.8525)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "b18a39bd-751f-4f6f-9bf2-f3dfff93b8d3")
	)
	(fp_line
		(start 8.827 2.54)
		(end 8.827 8.382)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "f1b216c4-5205-4507-9952-ba5990fad3ca")
	)
	(fp_line
		(start -8.825 2.54)
		(end 8.827 2.54)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "d0c71971-1939-4652-94aa-43ae274d28f3")
	)
	(fp_line
		(start -8.825 4.191)
		(end -8.825 2.54)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "8457eb15-645c-4e35-916a-650699a8f5a4")
	)
	(fp_line
		(start 8.827 2.54)
		(end 8.827 4.318)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "000fd7b8-a50d-4baa-8c13-5d975fe9c4c5")
	)
	(pad "1" thru_hole rect
		(at -5 0)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "7c78a4e2-484c-4909-947c-7011b535672d")
	)
	(pad "2" thru_hole circle
		(at -3 0)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "ae86a604-dc47-46fa-adce-b2c5740266e4")
	)
	(pad "3" thru_hole circle
		(at -1 0)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "4a9a49bc-a645-4997-947e-ac0cfd4ef5f2")
	)
	(pad "4" thru_hole circle
		(at 1 0)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "32e1ac24-5789-4a33-957a-eec037d4192d")
	)
	(pad "5" thru_hole circle
		(at 3 0)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "ca54dca3-3d2c-41d3-b5ed-fb9ea0400512")
	)
	(pad "6" thru_hole circle
		(at 5 0)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "979a8376-28e4-4ffd-8ee3-8513d02633ce")
	)
	(pad "7" thru_hole circle
		(at 8.125 0)
		(size 3.5 3.5)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "323cc39a-0f85-491e-8ed1-f6deda87ec05")
	)
	(pad "8" thru_hole circle
		(at -8.125 0)
		(size 3.5 3.5)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "f11d99df-a915-4dc8-876b-0f95cd767354")
	)
	(embedded_fonts no)
)
