(footprint "SPARK_GAP"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 0 0)
		(layer "F.SilkS")
		(uuid "37cfcc88-4a97-4576-b7d9-f492efbbb59a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" ""
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "3dce75ee-1bd3-44d3-bb9f-8285a939de4d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "86deb76b-ddc4-43ce-9fa8-5740cb970f2c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "2c5eb3dc-3c1b-46af-b9bc-6f03289f6cc8")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_poly
		(pts
			(xy -0.3 -0.15) (xy 0.3 -0.15) (xy 0.3 0.15) (xy -0.3 0.15)
		)
		(stroke
			(width 0)
			(type default)
		)
		(fill yes)
		(layer "F.Mask")
		(uuid "a4a452d7-a445-4b75-91c9-7751c783d02a")
	)
	(pad "1" smd circle
		(at -0.15 0.1)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 90)
		(uuid "e8e4449e-a651-4ced-bd4a-49e08730305f")
	)
	(pad "1" smd circle
		(at 0 0.1)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 90)
		(uuid "1586775b-8d44-46be-8099-8962c2892505")
	)
	(pad "1" smd rect
		(at 0 0.25)
		(size 0.5 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "aaaf947d-8a73-416f-b92e-dade7b2880fc")
	)
	(pad "1" smd circle
		(at 0.15 0.1)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 90)
		(uuid "4253efa1-d4d1-4d56-9785-7c4f6b689c02")
	)
	(pad "2" smd circle
		(at -0.15 -0.1 180)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 90)
		(uuid "21b502f1-0c83-45d2-a16b-8e83e02a2577")
	)
	(pad "2" smd rect
		(at 0 -0.25)
		(size 0.5 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "edccf633-8ede-41f1-ba94-c55dd0e8e666")
	)
	(pad "2" smd circle
		(at 0 -0.1 180)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 90)
		(uuid "a6ce5eaa-7eb6-4b7b-893e-6813bf7b1265")
	)
	(pad "2" smd circle
		(at 0.15 -0.1 180)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 90)
		(uuid "b55f0638-0798-4795-a464-0927f5d783a5")
	)
	(embedded_fonts no)
)
