(footprint "batt_con_nec"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 0 0)
		(layer "F.SilkS")
		(uuid "d8835094-b56a-475c-91c1-a66fa19958a8")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" ""
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "8759ecc4-e9f7-49a9-95a2-ba0920c850d7")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "c0668aee-3943-4dde-9f49-4b40aa5a53e3")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "0e025498-3b2a-464d-87c9-49dbc45037d4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_line
		(start -8.5 -2.25)
		(end -8.5 1.25)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "46858884-9865-4ee3-8ac8-998da03afe6e")
	)
	(fp_line
		(start -8.5 1.25)
		(end 8.5 1.25)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "a9fab256-5986-425b-9829-1944cad63b15")
	)
	(fp_line
		(start 8.5 -2.25)
		(end -8.5 -2.25)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "c74c7ac2-8dad-4a92-b976-6c373d512ef6")
	)
	(fp_line
		(start 8.5 1.25)
		(end 8.5 -2.25)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "968b047d-5104-447d-8bd7-4e8fcee6bcde")
	)
	(fp_line
		(start -6.5 -6.5)
		(end -6.5 -2.25)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "d1a0e45d-ac20-45c9-8164-8c280ca8d9dc")
	)
	(fp_line
		(start -6.25 -6.75)
		(end -6.5 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "9f519fee-41bb-4872-8191-04fb36c128aa")
	)
	(fp_line
		(start -6 -6.5)
		(end -6.25 -6.75)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "9dfb0b21-3340-44b3-ad36-db799a2ea50d")
	)
	(fp_line
		(start -5.988 -6.5)
		(end -6 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "33c09445-8e75-472a-9dc2-569a243fa4f7")
	)
	(fp_line
		(start -5.988 -2.25)
		(end -5.988 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "77388c40-9fd9-4b37-bae4-9c2cd94e49e4")
	)
	(fp_line
		(start -4 -6.5)
		(end -4 -2.25)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "585e8cff-342f-4ccc-acd7-1847a58e5a09")
	)
	(fp_line
		(start -3.75 -6.75)
		(end -4 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "2801cb1a-897b-489d-81e4-bcbabefe105d")
	)
	(fp_line
		(start -3.5 -6.5)
		(end -3.75 -6.75)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "87a3cf4c-6d8f-414d-9c67-aab2655c77f6")
	)
	(fp_line
		(start -3.488 -6.5)
		(end -3.5 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "3ea8ca0d-babb-44ab-8dff-c0c333d165b2")
	)
	(fp_line
		(start -3.488 -2.25)
		(end -3.488 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "2e6e2fd4-b14a-4bb8-a82c-d0214bc11e41")
	)
	(fp_line
		(start -1.5 -6.5)
		(end -1.5 -2.25)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "4333ebaa-71fc-4235-bb62-02996f3642b9")
	)
	(fp_line
		(start -1.25 -6.75)
		(end -1.5 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "2163bb1b-0b46-4885-a569-1682eb83d442")
	)
	(fp_line
		(start -1 -6.5)
		(end -1.25 -6.75)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "f7cc4543-3887-44ad-bb95-a0e5ede5f381")
	)
	(fp_line
		(start -0.988 -6.5)
		(end -1 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "3a9a5b52-c9e5-45a5-a12f-cce9c592f77d")
	)
	(fp_line
		(start -0.988 -2.25)
		(end -0.988 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "73c315d3-30a5-4a9e-96de-bc2187e13405")
	)
	(fp_line
		(start 1 -6.5)
		(end 1 -2.25)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "9c4db4e6-ecda-413b-a617-cdc0e6843b73")
	)
	(fp_line
		(start 1.25 -6.75)
		(end 1 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "4a13ff4a-1cc4-4c40-b34e-4c2aad4f095d")
	)
	(fp_line
		(start 1.5 -6.5)
		(end 1.25 -6.75)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "3c6e1728-08b1-4cf2-aa8d-f86bc4209c5c")
	)
	(fp_line
		(start 1.512 -6.5)
		(end 1.5 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "411f3d73-eaad-40b1-8372-a7faf9c02457")
	)
	(fp_line
		(start 1.512 -2.25)
		(end 1.512 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "a65302b3-efa8-4b51-bddd-14ee1167a8b4")
	)
	(fp_line
		(start 3.5 -6.5)
		(end 3.5 -2.25)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "675d7e9b-ad8a-4908-875c-686ebf2e2000")
	)
	(fp_line
		(start 3.75 -6.75)
		(end 3.5 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "60700fdf-33ad-416f-9305-59fc71e6fa8e")
	)
	(fp_line
		(start 4 -6.5)
		(end 3.75 -6.75)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "ab45f2e3-0ab3-47cf-8314-8488b6e6866f")
	)
	(fp_line
		(start 4.012 -6.5)
		(end 4 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "b02bd719-1c42-4e2b-b223-a9a5e48b3e0c")
	)
	(fp_line
		(start 4.012 -2.25)
		(end 4.012 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "4f71cb31-e471-43d5-b035-cee5a56fd16a")
	)
	(fp_line
		(start 6 -6.5)
		(end 6 -2.25)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "a47c433c-42b9-411e-ab89-8b751eec2c4e")
	)
	(fp_line
		(start 6.25 -6.75)
		(end 6 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "ebb8db3b-4fbe-4c7d-9135-a62a1ab5ce7b")
	)
	(fp_line
		(start 6.5 -6.5)
		(end 6.25 -6.75)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "3b5b8f3f-5818-489a-a644-a9c31c310666")
	)
	(fp_line
		(start 6.512 -6.5)
		(end 6.5 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "45e7e88d-489a-4a3c-886d-42ec65b9910f")
	)
	(fp_line
		(start 6.512 -2.25)
		(end 6.512 -6.5)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "56b30a24-b0f1-42f9-b8c7-cb897783b348")
	)
	(pad "1" thru_hole circle
		(at 6.25 0)
		(size 1.65 1.65)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "27afc56f-5d66-4062-9b4d-2b8988e28fe8")
	)
	(pad "2" thru_hole circle
		(at 3.75 0)
		(size 1.65 1.65)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "0f018e21-cd50-4fb7-b2e5-cb10f301e727")
	)
	(pad "3" thru_hole circle
		(at 1.25 0)
		(size 1.65 1.65)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "cd5a307f-e9a5-4d18-9c1e-9fcfb11ec837")
	)
	(pad "4" thru_hole circle
		(at -1.25 0)
		(size 1.65 1.65)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "1b3925d3-5cd8-4b33-adb6-f130122a594d")
	)
	(pad "5" thru_hole circle
		(at -3.75 0)
		(size 1.65 1.65)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "ef692fa2-bd6a-4c0f-8d7b-7ba63d681037")
	)
	(pad "6" thru_hole circle
		(at -6.25 0)
		(size 1.65 1.65)
		(drill 1.2)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "6382ae45-fdc7-4b38-a177-806acfee6c31")
	)
	(embedded_fonts no)
)
