(footprint "CONN-TH_SMTSOM2.550BTR_C5301778"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 0 0)
		(layer "F.SilkS")
		(uuid "dd4ea1b4-b037-4ecf-957b-afc13eaa43ca")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" ""
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "7be0a33c-908c-4101-8960-627d22fdcb18")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "1443e986-5f64-4ccd-801f-35c7b196c31e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "b5fc4f72-51d1-492f-9254-46ce0529a8d9")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "JLC_3DModel_Q" "d083a49ffadd43d38c30589efc30b4de"
		(at 0 0 0)
		(layer "Cmts.User")
		(hide yes)
		(uuid "b77edd1b-e49a-408d-bd07-8e51c3219c43")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "JLC_3D_Size" "5.56 5.561"
		(at 0 0 0)
		(layer "Cmts.User")
		(hide yes)
		(uuid "82a3cb76-230c-4d24-9b83-6daae3808c39")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 6.5 6.5)
		(drill 4.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "fdfee915-540a-4853-b46d-4ee7a4a85908")
	)
	(embedded_fonts no)
	(model "${KIPRJMOD}/EASYEDA_MODELS/CONN-TH_SMTSOM2.550BTR_C5301778.step"
		(offset
			(xyz 0 0 -1.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -0 -0 -0)
		)
	)
)
