(footprint "Test-Point-0.5mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 0 0)
		(layer "F.SilkS")
		(uuid "78d09bef-b0be-4de6-8e35-3990afd7d00a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" ""
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "62b086a4-eae1-4628-9474-3ffc5f0a6b94")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "8d4eb989-39e9-41b9-8b3d-fc9742ce2d26")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "f8e360fb-8553-4436-8997-db723d2d2b68")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_circle
		(center 0 0)
		(end 0.381 0)
		(stroke
			(width 0.152)
			(type default)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "d8de5f9f-4609-418f-bc57-cc055430b7e9")
	)
	(pad "1" smd circle
		(at 0 0)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 90)
		(uuid "676e9f4e-76d5-4e35-b599-2586a45e0a07")
	)
	(embedded_fonts no)
)
