(footprint "SPARK_GAP"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 0 0)
		(layer "F.SilkS")
		(uuid "c63b4e59-d441-42cf-afe0-9ec96a8f8969")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" ""
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "ea3debca-1b5b-44ea-a0f9-86c9db2f87b4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "33355727-d3b8-47fc-9f03-fe2ea6105ab2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "8c259050-9547-4384-a15f-9c3c8f7436db")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_poly
		(pts
			(xy -0.3 -0.15) (xy 0.3 -0.15) (xy 0.3 0.15) (xy -0.3 0.15)
		)
		(stroke
			(width 0)
			(type default)
		)
		(fill yes)
		(layer "F.Mask")
		(uuid "1a891e4e-48f1-4ccd-b32d-26693a10be30")
	)
	(pad "1" smd circle
		(at -0.15 0.1)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 90)
		(uuid "05988429-bebc-4fcc-904d-3bdc4c1f480e")
	)
	(pad "1" smd circle
		(at 0 0.1)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 90)
		(uuid "3123d41b-b277-433e-8a18-6a347c4f5ac8")
	)
	(pad "1" smd rect
		(at 0 0.25)
		(size 0.5 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "4159c2d4-e4cb-4066-aab6-f0b0c863ba22")
	)
	(pad "1" smd circle
		(at 0.15 0.1)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 90)
		(uuid "fa6ef2d1-7af6-442c-b41a-22f1bf98a0c2")
	)
	(pad "2" smd circle
		(at -0.15 -0.1 180)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 90)
		(uuid "5febadf8-5715-49d9-a231-91bf3f612848")
	)
	(pad "2" smd rect
		(at 0 -0.25)
		(size 0.5 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "60444b2e-d601-4403-b82a-548c5d4d4f3b")
	)
	(pad "2" smd circle
		(at 0 -0.1 180)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 90)
		(uuid "15221362-ae38-43c9-9369-2186f8448acf")
	)
	(pad "2" smd circle
		(at 0.15 -0.1 180)
		(size 1.524 1.524)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(thermal_bridge_angle 90)
		(uuid "f86426c2-761a-4005-8f57-fea30fc7d61c")
	)
	(embedded_fonts no)
)
