(footprint "CONN-TH_KH-A01M-A-M2-6P"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 0 0)
		(layer "F.SilkS")
		(uuid "ddbf58a1-8a2a-4ec7-a6f2-e8124fb374d7")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" ""
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "8e2b5fe2-ea53-43eb-97a3-22c18f4a6c85")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "3d92bcf8-ecff-4b56-8d90-83af9f937c9f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "38cc5988-169d-4d87-ab62-6dcdab171a7d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_line
		(start -8.827 -2.159)
		(end -8.827 -1.8525)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "5f9a1f68-c5e1-4ad8-87e4-ab7b37612132")
	)
	(fp_line
		(start -8.827 1.8525)
		(end -8.827 8.382)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "78a250b3-21f7-4b42-86ac-323e3110acde")
	)
	(fp_line
		(start -8.827 2.54)
		(end -8.827 3.175)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "99058f03-356d-4c91-a09a-e74f04e4790c")
	)
	(fp_line
		(start -8.827 8.382)
		(end 8.827 8.382)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "cba7d2c5-fc65-43ec-9687-ddd9617fc861")
	)
	(fp_line
		(start 8.827 -2.159)
		(end -8.827 -2.159)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "e9a7a50d-5b35-45dd-9fa7-4d4540d4519e")
	)
	(fp_line
		(start 8.827 -1.8525)
		(end 8.827 -2.159)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "dbc244bc-58b3-46dd-807e-9d4ac51354aa")
	)
	(fp_line
		(start 8.827 2.54)
		(end 8.827 1.8525)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "354960b3-e269-424c-b401-9c23b7219e19")
	)
	(fp_line
		(start 8.827 2.54)
		(end 8.827 8.382)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "6972b409-1f7b-4736-99eb-318796fb9863")
	)
	(fp_line
		(start -8.825 2.54)
		(end 8.827 2.54)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "30383964-452e-4052-877f-a06fc57de54c")
	)
	(fp_line
		(start -8.825 4.191)
		(end -8.825 2.54)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "de80acfc-f51e-4be0-9501-1d033e02f522")
	)
	(fp_line
		(start 8.827 2.54)
		(end 8.827 4.318)
		(stroke
			(width 0.254)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "a393df7e-dcda-438e-82a3-b4866f4db730")
	)
	(pad "1" thru_hole rect
		(at -5 0)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "73b38ef3-f5bd-4c96-8aeb-4bb4ec31e71f")
	)
	(pad "2" thru_hole circle
		(at -3 0)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "cbf2bfec-81ea-411c-b4eb-737dcd32d56b")
	)
	(pad "3" thru_hole circle
		(at -1 0)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "d1123a89-004b-4a47-a951-3ac86819a978")
	)
	(pad "4" thru_hole circle
		(at 1 0)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "ec72fe23-cc29-493a-807a-cea477eefc17")
	)
	(pad "5" thru_hole circle
		(at 3 0)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "0522284b-283c-4c11-a075-81f360c0f72c")
	)
	(pad "6" thru_hole circle
		(at 5 0)
		(size 1.6 1.6)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "5d862df3-00af-482b-bb0c-a4e1e0b4c8bf")
	)
	(pad "7" thru_hole circle
		(at 8.125 0)
		(size 3.5 3.5)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "e1aeb04d-c519-4206-adb7-31fc6f086c2d")
	)
	(pad "8" thru_hole circle
		(at -8.125 0)
		(size 3.5 3.5)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "12b60cf4-0a7a-4fdb-8c11-513644f3e270")
	)
	(embedded_fonts no)
)
